Cisco VPN v5.0.07.0440  (x64)
Windows 7, 10, Server 2012

1.)  Install SonicWALL Global VPN Client first
       GVCSetup64-v4.9.22.0822.exe

2.)  Install Cisco VPN x64 v5.0.07.0440

3.)  Error:  Secure VPN Connection Terminated locally by the Client.
     Reason 442: Failed to enable Virtual Adapter

     a.) HKEY_LOCAL_MACHINE\SYSTEM\CurrentControlSet\Services\CVirta 
     b.) Display Name = Cisco Systems VPN Adapter for 64-bit Windows
	 Display Name = Cisco Systems VPN Adapter  (x86)



Enable Split Tunneling

  ASDM
  
  Configuration > VPN > Group Policies
    *May have to apply to multiple policies

  Uncheck Inherit for Split Tunnel Policy
    Select Tunnel Network List Below

  Uncheck Inherit for Split Tunnel Network List
    Click Manage
      Click Add ACL, Provide name for ACL
      Click Add ACE
	Permit
	IP Address of remote network  (i.e. 192.168.0.0)
	Netmask  255.255.255.0
	OK
    Select newly created ACL for Split Tunnel Network List

  OK

  Apply

  Save


http://www.cisco.com/c/en/us/support/docs/security/asa-5500-x-series-next-generation-firewalls/70917-asa-split-tunnel-vpn-client.html

Document ID:70917